CAN2Web Professional
CAN-Ethernet Gateway
by

Hardware I: with SCB9328: 200MHz 32-Bit ARM9 CPU 16MB Flash-ROM 16MB SD-RAM 10/100MBit Ethernet-Interface 1 MBit CAN-Bus (galvanically isolated) 1 RS232-Linux-Terminal-Interface 2 USB Host-Ports 4 LEDs | Hardware II: with SCB9324 (WLAN): 200MHz 32-Bit ARM9 CPU 16MB Flash-ROM 16MB SD-RAM 512MB NAND Flash-Disk 10/100MBit Ethernet-Interface Onboard-WLAN for IEEE802.11b/g 1 MBit CAN-Bus (galvanically isolated) 1 RS232-Linux-Terminal-Interface 2 USB Host-Ports 4 LEDs | OnBoard Software: Linux 2.6.31 CAN-Ethernet-Gateway-SW "can2web.exe" including: Web-Server Web-Interface Datastream-Interface Command-Interface Linux-CAN-Driver | Configuration: Webbrowser Firefox Explorer ... DeviLANControl for MS Windows(PC)

© synertronixx